	Name
	Size (bytes)
	Description

	Synchronization bytes (0x46, 0x42)
	2
	Each data packet starts with SYNC bytes, that indicates a begin of data packet

	Serial number of GPS tracking device (ID)
	2
	from 0x0000 to 0xFFFF

	Number of events
	1
	This indicates how many events are in the current data packet. Value from no 0x01 up to 0x28

	Latitude
	4
	GPS position (Latitude) in degrees

	Longitude
	4
	GPS position (Longitude) in degrees

	UNIX time stamp
	4
	UNIX time stamp in seconds

	Speed (km/h)
	1
	from 0x00 up to 0xFF

	Fuel level/Number of pulses
	2
	In case if fuel sensor is connected (or analog input used), this value indicated a digital converter result, can be from 0x0000 up to 0x0FFF
In case if flow meter connected, this value
indicates a number of pulses from last event.
Value can be from 0x0000 up to 0xFFFF.

	Device STATUS register
	1
	Indicates status of digital inputs/outputs as
well as additional triggers. For detailed
information, see next table.



	Bit
	Name
	Description

	0
	IGNITION
	0 = OFF
1 = ON

	1
	DIGITAL INPUT 1
	0 = OFF
1 = ON

	2
	RESERVED
	0 = NOT RUNNING
1 = ENGINE RUNNING

	3
	DIGITAL OUTPUT 1
	0 = OFF
1 = ON

	5
	RESERVED
	

	6
	GPS JAMMER DETECTOR
	0 – normal mode
1 – GPS signal jammed

	7
	FUEL THEFT ALARM
	0 = No alarm
1 = Fuel theft detected
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